Node Details

NetApp HCI Configuration Compute Nodes

	SMALL
H300E	MEDIUM
H500E	LARGE
H700E	
RU	1RU, half-width	1RU, half-width	1RU, half-width	
Cores for VMs	16	24	36	
CPU	E5-2620 v4: 8C at 2.1GHz	E5-2650 v4: 12C at 2.2GHz	E5-2695 v4: 18C at 2.1GHz	
Memory	384GB	512GB	768GB	
Boot Device	1 x 240GB MLC	1 x 240GB MLC	1 x 240GB MLC	
Base Networking**	2 25/10GbE SFP28 /SFP+
2 1GbE RJ45	2 25/10GbE SFP28 /SFP+
2 1GbE RJ45	2 25/10GbE SFP28 /SFP+
2 1GbE RJ45	

NetApp HCI Configuration Storage Nodes

	SMALL
H300S	MEDIUM
H500S	LARGE
H700S	
RU	1RU, half-width	1RU, half-width	1RU, half-width	
CPU	E5-2620 v4: 8C at 2.1GHz	E5-2650 v4: 12C at 2.2GHz	E5-2695 v4: 18C at 2.1GHz	
Boot Device	1 x 240GB MLC 	1 x 240GB MLC 	1 x 240GB MLC	
Base Networking	2 25/10GbE SFP28 /SFP+
2 1GbE RJ45	2 25/10GbE SFP28 /SFP+
2 1GbE RJ45	2 25/10GbE SFP28 /SFP+
2 1GbE RJ45	
SSD	6 x 480GB	6 x 960GB	6 x 1.9TB	
Effective Block Capacity*	5.5TB – 11TB	11TB – 22TB	22TB – 44TB	

Power & Dimensions (per Chassis)

Rack Units	2 RU	
HCI Nodes	Mix and match four HCI nodes per chassis	
Power Input	220-240 V AC 
1 + 1 redundant ***
	
Max Watts / Current Per Power Supply	2200 W / 220-240 V / 12-11 A	
Node Physical Dimensions	39.20 mm / 1.54 in H
196.25 mm / 7.73 in W
587.55 mm / 23.13 in D
~ 3.60 kg / 8.0 lbs
	
Chassis Physical Dimensions	8.80 cm / 3.46 in H
44.70 cm / 17.60 in  W
73.00 cm / 28.74 in D
~ 24.70  kg / 54.45 lbs

Environmentals

Operating temperature, altitude, and relative humidity
	10° C to 35° C (50° F to 95° F); at <= 914.40m (at <= 3,000ft) elevation; 1° C derating per 1,000ft;
8% to 90% relative humidity, noncondensing
	
Non-Operating temperature and relative humidity
	-40° C to 70° C (-40° F to 158° F)	
Heat Dissipation	Typical BTU/hr — Small 2,730; Medium 3,412; Large 4,129
Worst Case BTU/hr — Small 3,856; Medium 4,982; Large 6,142
	
Certifications	FCC, UL, IEC 60950-1, CE, VCCI, KCC, SABS LOA (South Africa), BSMI, SONCAP, KEBS, KSA, TBS, UNGS

* NetApp HCI effective capacity calculation accounts for Helix data protection, system overhead, and global efficiencies including compression, deduplication, and thin provisioning. NetApp HCI customers typically achieve an effective capacity range of 5x to 10x the (usable) capacity, depending on application workloads.
** Cables and transceivers not included. Please refer HCI Network Compatibility document for more details.
***Certain configurations support 100-120 V.